BANDSAW - STEPS

PPE

TIMBER CHECKED - Metal/Gravel/etc.

WORK AREA CLEAR/SAFE – No tools/etc.

BLADE TENSIONED/TRACKED

GUARDS IN PLACE

GUIDES SET AND IN PLACE

SURROUNDING AREA SAFE

DUST EXTRACTOR – ON

START MACHINE

DOUBTS?? ASK