TABLE SAW - STEPS

PPE – Push Stick / Block at hand

TIMBER CHECKED - Metal/Gravel/etc.

WORK AREA CLEAR/SAFE – No tools/etc.

BLADE HEIGHT SET

BLADE SLOPE SET

GUARDS IN PLACE

GUIDES SET AND IN PLACE

SURROUNDING AREA SAFE

DUST EXTRACTOR – ON

ISOLATORS (2) - ON

EMERGENCY STOP BUTTON SET

START MACHINE

DOUBTS?? ASK