THICKNESSER/PLANER - STEPS

PPE

TIMBER CHECKED - Metal/Gravel/etc.

WORK AREA CLEAR/SAFE – No tools/etc.

PLANER SETUP

THICKNESSER SETUP

GUARDS IN PLACE

THICKNESSER/PLANER LEVER

GUIDE SET AND IN PLACE

SURROUNDING AREA SAFE

DUST EXTRACTOR – ON

EMERGENCY STOP BUTTON SET

START MACHINE

DOUBTS?? ASK